{"text_format":"2","workbook":"xls","n_sheets":8,"sheets":["Cohesion","Gravity","Density","WaterTable","Thickness","Slope","InternalFriction","NoParameters"],"not_rendered":{"charts":7,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Cohesion","index":0,"n_rows":24,"n_cols":11,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,null,"F = c+ (g-gwm)hcos2Qtanf",null,29368.91749701]
[null,null,null,"           (ghcosQ sinQ)",null,20784609.690826524,"(g = rg)"]
["Ranges"]
[12000,25,3200,1000,0,0.5,0.1,5]
[0,5,1200,1000,1,10,45,45]
["cohesion (c) (kg/m s2)","gravity (g) (m/s2)","Density overbunden (r) (kg/m3)","Density water (rw) (kg/m3)","Water table (m) (fraction of h)","Slab thickness (h) (m)","Slope angle (Q) (°)","Internal angle of friction (f)       (°)","Driving Forces","Resisting Forces","Factor of Safety"]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[]
[{"$nulls":9},"Cohesion values for"]
[{"$nulls":9},"Conifers","900 to 4400"]
[{"$nulls":9},"Alder","2000 to 12000"]
[{"$nulls":9},"Birch","1500 to 9000"]
[{"$nulls":9},"Poplar","2000 to 9000"]
[{"$nulls":9},"Clover","100 to 2000"]

{"sheet":"Gravity","index":1,"n_rows":29,"n_cols":11,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,null,"F = c+ (g-gwm)hcos2Qtanf",null,29368.91749701]
[null,null,null,"           (ghcosQ sinQ)",null,20784609.690826524,"(g = rg)"]
["Ranges"]
[12000,25,3200,1000,0,0.5,0.1,5]
[0,0.5,1200,1000,1,10,45,45]
["cohesion (c) (kg/m s2)","gravity (g) (m/s2)","Density overbunden (r) (kg/m3)","Density water (rw) (kg/m3)","Water table (m) (fraction of h)","Slab thickness (h) (m)","Slope angle (Q) (°)","Internal angle of friction (f)       (°)","Driving Forces","Resisting Forces","Factor of Safety"]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[]
[{"$nulls":9},"Gravity on"]
[{"$nulls":9},"Mercury",3.59]
[{"$nulls":9},"Venus",8.87]
[{"$nulls":9},"Earth",9.81]
[{"$nulls":9},"Moon",1.67]
[{"$nulls":9},"Mars",3.77]
[{"$nulls":9},"Jupiter",26]
[{"$nulls":9},"Saturn",11.1]
[{"$nulls":9},"Uranus",10.7]
[{"$nulls":9},"Neptune",14.1]
[{"$nulls":9},"Pluto",0.42]

{"sheet":"Density","index":2,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,null,"F = c+ (g-gwm)hcos2Qtanf",null,29368.91749701]
[null,null,null,"           (ghcosQ sinQ)",null,20784609.690826524,"(g = rg)"]
["Ranges"]
[12000,25,3200,1000,0,0.5,0.1,5]
[0,5,1200,1000,1,10,45,45]
["cohesion (c) (kg/m s2)","gravity (g) (m/s2)","Density overbunden (r) (kg/m3)","Density water (rw) (kg/m3)","Water table (m) (fraction of h)","Slab thickness (h) (m)","Slope angle (Q) (°)","Internal angle of friction (f)       (°)","Driving Forces","Resisting Forces","Factor of Safety"]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]

{"sheet":"WaterTable","index":3,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,null,"F = c+ (g-gwm)hcos2Qtanf",null,29368.91749701]
[null,null,null,"           (ghcosQ sinQ)",null,20784609.690826524,"(g = rg)"]
["Ranges"]
[12000,25,3200,1000,0,0.5,0.1,5]
[0,5,1200,1000,1,10,45,45]
["cohesion (c) (kg/m s2)","gravity (g) (m/s2)","Density overbunden (r) (kg/m3)","Density water (rw) (kg/m3)","Water table (m) (fraction of h)","Slab thickness (h) (m)","Slope angle (Q) (°)","Internal angle of friction (f)       (°)","Driving Forces","Resisting Forces","Factor of Safety"]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]

{"sheet":"Thickness","index":4,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,null,"F = c+ (g-gwm)hcos2Qtanf",null,29368.91749701]
[null,null,null,"           (ghcosQ sinQ)",null,20784609.690826524,"(g = rg)"]
["Ranges"]
[12000,25,3200,1000,0,0.5,0.1,5]
[0,5,1200,1000,1,10,45,45]
["cohesion (c) (kg/m s2)","gravity (g) (m/s2)","Density overbunden (r) (kg/m3)","Density water (rw) (kg/m3)","Water table (m) (fraction of h)","Slab thickness (h) (m)","Slope angle (Q) (°)","Internal angle of friction (f)       (°)","Driving Forces","Resisting Forces","Factor of Safety"]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]

{"sheet":"Slope","index":5,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,null,"F = c+ (g-gwm)hcos2Qtanf",null,29368.91749701]
[null,null,null,"           (ghcosQ sinQ)",null,20784609.690826524,"(g = rg)"]
["Ranges"]
[12000,25,3200,1000,0,0.5,0.1,5]
[0,5,1200,1000,1,10,50,45]
["cohesion (c) (kg/m s2)","gravity (g) (m/s2)","Density overbunden (r) (kg/m3)","Density water (rw) (kg/m3)","Water table (m) (fraction of h)","Slab thickness (h) (m)","Slope angle (Q) (°)","Internal angle of friction (f)       (°)","Driving Forces","Resisting Forces","Factor of Safety"]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]

{"sheet":"InternalFriction","index":6,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,null,"F = c+ (g-gwm)hcos2Qtanf",null,29368.91749701]
[null,null,null,"           (ghcosQ sinQ)",null,20784609.690826524,"(g = rg)"]
["Ranges"]
[12000,25,3200,1000,0,0.5,0.1,5]
[0,5,1200,1000,1,10,45,55]
["cohesion (c) (kg/m s2)","gravity (g) (m/s2)","Density overbunden (r) (kg/m3)","Density water (rw) (kg/m3)","Water table (m) (fraction of h)","Slab thickness (h) (m)","Slope angle (Q) (°)","Internal angle of friction (f)       (°)","Driving Forces","Resisting Forces","Factor of Safety"]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[9000,9.8,1600,1000,0.4,4,30,30,29368.91749701,27158.55666268,1.0813872718562902]
[]
[]
[{"$nulls":9},"Friction angles for "]
[{"$nulls":9},"Sand","28 to 46"]
[{"$nulls":9},"Gravel","34 to 48"]
[{"$nulls":9},"Broken Rock","30 to 50"]
[{"$nulls":9},"Clay","7 to 27"]
[{"$nulls":9},"Glacial Clay ","27 to 35"]
[{"$nulls":9},"Rock","25 to 45"]

{"sheet":"NoParameters","index":7,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,null,"F = c+ (g-gwm)hcos2Qtanf",null,33785.70444178667]
[null,null,null,"           (ghcosQ sinQ)",null,10392304.845413262,"(g = rg)"]
["Ranges"]
[100000,25,3200,1000,0,0.5,0.1,5]
[0,5,1200,1000,1,10,45,45]
["cohesion (c) (kg/m s2)","gravity (g) (m/s2)","Density overbunden (r) (kg/m3)","Density water (rw) (kg/m3)","Water table (m) (fraction of h)","Slab thickness (h) (m)","Slope angle (Q) (°)","Internal angle of friction (f)       (°)","Driving Forces","Resisting Forces","Factor of Safety"]
[0,9.8,1600,1000,0,4,15,30,33785.70444178667,15680.000000000002,2.154700538379252]
[0,9.8,1600,1000,0,4,15,30,33785.70444178667,15680.000000000002,2.154700538379252]
[0,9.8,1600,1000,0,4,15,30,33785.70444178667,15680.000000000002,2.154700538379252]
[0,9.8,1600,1000,0,4,15,30,33785.70444178667,15680.000000000002,2.154700538379252]
[0,9.8,1600,1000,0,4,15,30,33785.70444178667,15680.000000000002,2.154700538379252]
[0,9.8,1600,1000,0,4,15,30,33785.70444178667,15680.000000000002,2.154700538379252]
[0,9.8,1600,1000,0,4,15,30,33785.70444178667,15680.000000000002,2.154700538379252]
[0,9.8,1600,1000,0,4,15,30,33785.70444178667,15680.000000000002,2.154700538379252]
[0,9.8,1600,1000,0,4,15,30,33785.70444178667,15680.000000000002,2.154700538379252]
[0,9.8,1600,1000,0,4,15,30,33785.70444178667,15680.000000000002,2.154700538379252]
[0,9.8,1600,1000,0,4,15,30,33785.70444178667,15680.000000000002,2.154700538379252]