STEP BY STEP
1. LOG IN 

2. GO TO START (BOTTOM LEFT CORNER)

3. FIND MY COMPUTER AND CLICK ON 

4. GO TO LOCAL DISC C: DRIVE

5. OPEN ESRI FOLDER

6. OPEN AEJEE FOLDER

7. OPEN DATA FOLDER

8. FIND SHADOWS FOLDER

LOOK AT THE 4 jpg.PHOTO IMAGES

CLOSE THE FOLDERS AND RETURN TO THE DESKTOP

NEXT:

1. GO TO PROGRAMS ON THE DESKTOP

2. OPEN IMAGEJ (THE MICROSCOPE ICON)

3. A TOOL BAR APPEARS

4. MOVE MOUSE OVER THE TOOL BAR TO REVEAL WHAT EACH TOOL IS

5. GO TO FILE---OPEN---CHOOSE IMAGE 1
6. REPEAT UNTIL YOU HAVE ALL FOUR (4) IMAGES OPEN

7. OPEN IMAGE---STACKS---CONVERT IMAGES TO STACKS

8. WE WILL DO MORE WITH THIS LATER

9. OPEN IMAGE---STACKS---CONVERT STACK TO IMAGES

10. USING THE STRAIGHT LINE TOOL---OPEN ONE IMAGES AT A TIME

11. DRAW A LINE FROM ONE END OF THE SHADOW TO THE OTHER

12. OPEN ANALYZE---SET MEASUREMENT---AREA IS CHECKED—ONE DECIMAL PLACE

13. OPEN ANALYZE---MEASURE AND WAIT FOR RESULTS
14. REPEAT WITH EACH IMAGE

OPEN—ANALYZE—MEASURE—RESULTS

15. COMPARE THE RESULTS WITH OUR MEASUREMENTS

