{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":18,"n_cols":3,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Factor of Safety Spreadsheet"]
["Variable","Value","Units"]
["Cohesion",1100,"N/m2"]
["Density of Regolith",2200,"kg/m3"]
["Depth of Regolith",10,"m"]
["Angle of Internal Friction",15,"degrees"]
["Slope",14,"degrees"]
["Depth of water",0]
[]
["Constant","Value","Units"]
["Gravity",9.8,"m/s2"]
["Density of Water",1000,"kg/m3"]
[]
[]
["Shear Strength"]
["Shear Stress"]
[]
["Factor of Safety"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}