{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":9,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["DATA ON BUILDING"]
[]
["Area (sqft)",1072]
["Year built",1984]
["N. of residents",4]
["Heating type ","Natural Gas","(e.g., electric, natural gas, wood)"]
["Air conditioning? ","Y","(Y/N)"]
[]
["DATA LOG"]
[null,null,null,"METER READINGS",null,null,"CONSUMPTION"]
["Month","Day","Hour","Natural gas","Electricity","Water","Natural gas","Electricity","Water"]
[null,null,null,"(x100 cubic feet)","(kWh)","(x100 cubic feet)","(x100 cubic feet)","(kWh)","(x100 cubic feet)"]
[]
[2,6,1400,135500,53305]
[2,8,1700,136800,53345,null,1300,40,0]
[2,13,1500,137200,53452,null,400,107]
[2,14,1500,137500,53570,null,300,118]
[2,15,1700,138800,53599,null,1300,29]
[2,19,2000,138800,53694,null,0,95]
[2,20,1530,139000,53700,null,200,6]
[2,24,2100,139600,53718,null,600,18]
[2,25,2100,139800,53719,null,200,1]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}