{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["Chart1","Pueblo.txt"],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"Chart1","index":0,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"Pueblo.txt","index":1,"n_rows":146,"n_cols":6,"rows_kept":146,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["#"]
["# U.S. Geological Survey"]
["# National Water Information System"]
["# Retrieved: 2002-09-09 19:31:40 EDT"]
["#"]
["# ---------------------WARNING---------------------"]
["# The data you have obtained from this automated"]
["# U.S. Geological Survey database have not received"]
["# Director's approval and as such are provisional"]
["# and subject to revision.  The data are released"]
["# on the condition that neither the USGS nor the"]
["# United States Government may be held liable for"]
["# any damages resulting from its use."]
["#"]
["# This file contains the annual peak streamflow data."]
["#"]
["# This information includes the following fields:"]
["#"]
["#  agency_cd     Agency Code"]
["#  site_no       USGS station number"]
["#  peak_dt       format YYYY-MM-DD"]
["#  peak_va       Annual peak streamflow value in cfs"]
["#  peak_cd       Peak Discharge-Qualification codes (see explanation below)"]
["#  gage_ht       Gage height for the associated peak streamflow in feet"]
["#  gage_ht_cd    Gage height qualification codes"]
["#  year_last_pk  Peak streamflow reported is the highest since this year "]
["#  ag_dt         Date of maximum gage-height for water year (if not concurrent with peak)"]
["#  ag_tm         Time of maximum gage-height for water year (if not concurrent with peak"]
["#  ag_gage_ht    maximum Gage height for water year in feet (if not concurrent with peak"]
["#  ag_gage_ht_cd maximum Gage height code"]
["#"]
["# Sites in this file include:"]
["#  USGS 07099500 ARKANSAS RIVER NEAR PUEBLO, CO."]
["#"]
["# Peak Streamflow-Qualification Codes(peak_cd):"]
["#   1 ... Discharge is a Maximum Daily Average"]
["#   2 ... Discharge is an Estimate"]
["#   3 ... Discharge affected by Dam Failure"]
["#   4 ... Discharge less than indicated value,"]
["#           which is Minimum Recordable Discharge at this site"]
["#   5 ... Discharge affected to unknown degree by"]
["#           Regulation or Diversion"]
["#   6 ... Discharge affected by Regulation or Diversion"]
["#   7 ... Discharge is an Historic Peak"]
["#   8 ... Discharge actually greater than indicated value"]
["#   9 ... Discharge due to Snowmelt, Hurricane,"]
["#           Ice-Jam or Debris Dam breakup"]
["#   A ... Year of occurrence is unknown or not exact"]
["#   B ... Month or Day of occurrence is unknown or not exact"]
["#   C ... All or part of the record affected by Urbanization,"]
["#            Mining, Agricultural changes, Channelization, or other"]
["#   D ... Base Discharge changed during this year"]
["#   E ... Only Annual Maximum Peak available for this year"]
["#"]
["# Gage height qualification codes(gage_ht_cd,ag_gage_ht_cd):"]
["#   1 ... Gage height affected by backwater"]
["#   2 ... Gage height not the maximum for the year"]
["#   3 ... Gage height at different site and(or) datum"]
["#   4 ... Gage height below minimum recordable elevation"]
["#   5 ... Gage height is an estimate"]
["#   6 ... Gage datum changed during this year"]
["#"]
["#"]
["agency_cd","site_no","peak_dt","rank","ri","peak_va"]
["5s","15s","10d","6s",null,"8s"]
["USGS",7099500,"1895-07-31",1,82,103000]
["USGS",7099500,"1896-08-18",2,41,30000]
["USGS",7099500,"1897-06-02",3,27.33333333,25600]
["USGS",7099500,"1898-07-13",4,20.5,23500]
["USGS",7099500,"1899-08-14",5,16.4,17000]
["USGS",7099500,"1900-05-20",6,13.66666667,16500]
["USGS",7099500,"1901-05-21",7,11.71428571,12800]
["USGS",7099500,"1902-08-05",8,10.25,12400]
["USGS",7099500,"1903-06-09",9,9.111111111,11200]
["USGS",7099500,"2004-08-15",10,8.2,11200]
["USGS",7099500,"2005-08-06",11,7.454545455,11100]
["USGS",7099500,"2006-06-13",12,6.833333333,11100]
["USGS",7099500,"2007-07-28",13,6.307692308,11000]
["USGS",7099500,"2008-08-01",14,5.857142857,10900]
["USGS",7099500,"2009-08-18",15,5.466666667,10600]
["USGS",7099500,"2010-07-29",16,5.125,10500]
["USGS",7099500,"2011-05-28",17,4.823529412,10500]
["USGS",7099500,"2012-07-31",18,4.555555556,10500]
["USGS",7099500,"2013-07-23",19,4.315789474,10300]
["USGS",7099500,"2014-08-03",20,4.1,10200]
["USGS",7099500,"2015-06-24",21,3.904761905,9880]
["USGS",7099500,"2016-06-17",22,3.727272727,9600]
["USGS",7099500,"2017-06-19",23,3.565217391,9300]
["USGS",7099500,"2018-06-23",24,3.416666667,9300]
["USGS",7099500,"2019-09-04",25,3.28,9290]
["USGS",7099500,"2020-07-18",26,3.153846154,9070]
["USGS",7099500,"2021-06-03",27,3.037037037,8900]
["USGS",7099500,"2022-08-06",28,2.928571429,8850]
["USGS",7099500,"2023-07-12",29,2.827586207,8800]
["USGS",7099500,"2024-06-15",30,2.733333333,8700]
["USGS",7099500,"2025-07-03",31,2.64516129,8630]
["USGS",7099500,"2026-06-14",32,2.5625,8500]
["USGS",7099500,"2027-07-22",33,2.484848485,8500]
["USGS",7099500,"2028-07-21",34,2.411764706,8400]
["USGS",7099500,"2029-07-28",35,2.342857143,8360]
["USGS",7099500,"1930-08-28",36,2.277777778,8010]
["USGS",7099500,"1931-09-01",37,2.216216216,8000]
["USGS",7099500,"1932-06-26",38,2.157894737,7800]
["USGS",7099500,"1933-08-02",39,2.102564103,7800]
["USGS",7099500,"1934-08-03",40,2.05,7600]
["USGS",7099500,"1935-05-18",41,2,7600]
["USGS",7099500,"1936-05-24",42,1.952380952,7560]
["USGS",7099500,"1937-08-29",43,1.906976744,7500]
["USGS",7099500,"1938-08-26",44,1.863636364,7500]
["USGS",7099500,"1939-06-01",45,1.822222222,7280]
["USGS",7099500,"1940-08-19",46,1.782608696,7050]
["USGS",7099500,"1941-07-19",47,1.744680851,6800]
["USGS",7099500,"1942-06-08",48,1.708333333,6770]
["USGS",7099500,"1943-08-18",49,1.673469388,6760]
["USGS",7099500,"1944-07-05",50,1.64,6620]
["USGS",7099500,"1945-08-14",51,1.607843137,6600]
["USGS",7099500,"1946-08-27",52,1.576923077,6510]
["USGS",7099500,"1947-07-09",53,1.547169811,6300]
["USGS",7099500,"1948-06-13",54,1.518518519,6300]
["USGS",7099500,"1949-06-06",55,1.490909091,6100]
["USGS",7099500,"1950-07-26",56,1.464285714,6050]
["USGS",7099500,"1951-08-03",57,1.438596491,5980]
["USGS",7099500,"1952-06-08",58,1.413793103,5870]
["USGS",7099500,"1953-07-21",59,1.389830508,5800]
["USGS",7099500,"1954-06-30",60,1.366666667,5760]
["USGS",7099500,"1955-05-19",61,1.344262295,5260]
["USGS",7099500,"1956-08-01",62,1.322580645,5190]
["USGS",7099500,"1957-06-29",63,1.301587302,4930]
["USGS",7099500,"1958-06-05",64,1.28125,4740]
["USGS",7099500,"1959-06-17",65,1.261538462,4540]
["USGS",7099500,"1960-06-08",66,1.242424242,4520]
["USGS",7099500,"1961-08-02",67,1.223880597,4400]
["USGS",7099500,"1962-07-08",68,1.205882353,4380]
["USGS",7099500,"1963-08-14",69,1.188405797,4300]
["USGS",7099500,"1964-05-27",70,1.171428571,3860]
["USGS",7099500,"1965-08-22",71,1.154929577,3700]
["USGS",7099500,"1966-08-01",72,1.138888889,3560]
["USGS",7099500,"1967-07-18",73,1.123287671,3540]
["USGS",7099500,"1968-08-10",74,1.108108108,3360]
["USGS",7099500,"1969-08-23",75,1.093333333,3360]
["USGS",7099500,"1970-08-11",76,1.078947368,3320]
["USGS",7099500,"1971-06-07",77,1.064935065,2910]
["USGS",7099500,"1972-06-28",78,1.051282051,2840]
["USGS",7099500,"1973-07-30",79,1.037974684,2820]
["USGS",7099500,"1974-07-23",80,1.025,2580]
["USGS",7099500,"1975-07-10",81,1.012345679,2200]