{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[[0,0,0,9],[2,0,2,9]],"flags":["formulas_cached_only"]}
["Annotated Time-Log to Woburn Induced River Infiltration Animation"]
[{"$nulls":9}," "]
["Scott Bair, Geological Sciences, Ohio State University"]
[]
["Aberjona River Infiltration Animation (8 min, 7 seconds)"]
[]
["Time (sec)","Source Initiation"]
["00:00:00","1964-01-01","constant source of 100 ppb placed in all river cells, v. small dispersivity, no retardation"]
[]
["Time (sec)","Plan View"]
["00:00:00","1964-01-01","animation begins when only Riley Tannery wells are operating"]
["00:09:00","1964-10-01","well G on but river water doesn't reach well, flows back to river after G off in 12/65"]
["00:11:00","1964-12-01","maximum extent of infiltration due to well G being on for 3 months"]
["00:19:00","1966-03-01","river water gets to well G; notice length of Aberjona River influenced by well G"]
["00:59:00","1972-04-01","maximum extent with only well G on, some areas with 80% river water; now 27 "]
[null," ","months with no pumping at well G or H"]
["01:14:00","1974-08-01","slow flushing, some areas with 40-60% river water"]
["01:47:00","1979-05-01","maximum extent with both wells G and H pumping, not that much more river length"]
[null," ","influenced by pumping than when only well G pumped"]
["02:02:00","1985-12-01","still many areas with 20-60% river water, aquifer not quickly flushed"]
[]
["Time (sec)","Cross Section #1"]
["02:05:00","Preamble","geometry of well G, river, valley"]
["02:20:00","1966-03-01","note length of Aberjona River influenced by well G, which is < 20% river water"]
["02:32:00","1967-12-01","well G is 20-40% river water, which pervades aquifer from top-to-bottom (partial pene)"]
["03:00:00","1972-04-01","maximum extent of infiltration along Aberjona River with well G only, which is 20-40% "]
[null,null,"river water"]
["03:14:00","1974-07-01","slow flushing, still areas within aquifer that are 40-60% river water"]
["03:48:00","1979-05-01","well G is 40-60% river water; maximum extent of the > 80% river water zone"]
["04:04:00","1985-12-01","even after 6 years of flushing, some places in aquifer are still > 20% river water"]
[]
["Time (sec)","Cross Section #2"]
["04:07:00","Preamble","geometry of well H, river, valley"]
["04:28:00","1967-03-01","red zone of > 80% river water is moving not to well H, which is not yet built, but to well G"]
["04:34:00","1967-12-01","well H now on line and has been pumping for 6 months and is now producing 20-40%"]
[null,null,"river water; well H will not pump again for 6.75 years until August 1974 -- flushing occurs"]
["05:50:00","1979-05-01","well H pumping about 50% river water; flushing until December 1985"]
["06:05:00","1985-12-01","almost all river water flushed out of aquifer near well H"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}