{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["GLACPRO","Shape factor"],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":1,"defined_names":6,"comments":3,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"GLACPRO","index":0,"n_rows":34,"n_cols":10,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["  UPICE","BEDROCK"," SHAPE"," BASAL","Step",null,"Calculated","Centerline","MORAINE","Ice"]
["  DIST.","ELEVATION"," FACT."," SHEAR","Length","Change","Elevation","Thickness","CREST","Thickness"]
[" (ft)","   (ft)",null," (bar)"," (ft)"," (ft)"," (ft)"," (ft)"," (ft)"," (ft)"]
["---------","---------","---------","---------","---------","---------","---------","---------","---------","---------"]
[0,9760,{"$nulls":4},9760,0,9760,0]
[2000,9800,{"$nulls":4},9880,80,9880,80]
[4000,9800,{"$nulls":4},9960,160,9960,160]
[6000,9840,0.85,0.4,2000,130,10090,250,10080,240]
[8000,9860,0.8,0.5,2000,110.5,10200.5,340.5,10200,340]
[10000,9880,0.8,0.7,2000,113.58296622613803,10314.082966226139,434.0829662261385,10320,440]
[12000,9900,0.75,0.7,2000,95.03559582626453,10409.118562052403,509.1185620524029,10420,520]
[14000,9930,0.75,0.7,2000,81.02893197810214,10490.147494030505,560.1474940305052,10480,550]
[16000,10000,0.75,1,2000,105.21038469579206,10595.357878726298,595.3578787262977,10600,600]
[18000,10060,0.75,1,2000,98.98808000897658,10694.345958735274,634.3459587352736]
[20000,10080,0.7,1,2000,99.5400952324945,10793.886053967768,713.886053967768]
[22000,10100,0.7,1,2000,88.44948965161889,10882.335543619387,782.335543619387]
[24000,10120,0.7,1,2000,80.71070994772123,10963.046253567109,843.0462535671086]
[26000,10170,0.7,1,2000,74.89844937414317,11037.944702941251,867.9447029412513]
[28000,10220,0.7,1,2000,72.74986174681581,11110.694564688067,890.6945646880667]
[30000,10450,0.7,1,2000,70.89170591825788,11181.586270606325,731.5862706063253]
[32000,10560,0.7,1,2000,86.3095162933081,11267.895786899633,707.8957868996331]
[34000,10760,0.7,1,2000,89.19795584517256,11357.093742744806,597.0937427448061]
[36000,10920,0.7,1,2000,105.75032465185953,11462.844067396665,542.8440673966652]
[38000,11150,0.7,1,2000,116.31859116683984,11579.162658563506,429.16265856350583]
[40000,11400,0.7,1,2000,147.13036160743587,11726.293020170942,326.2930201709423]
[42000,11640,0.8,1,2000,169.32633119474934,11895.61935136569,255.61935136569082]
[43000,11800,0.8,1,1000,108.07084773671725,12003.690199102408,203.69019910240786]
[44000,11960,0.8,1,1000,135.6226275085095,12139.312826610918,179.3128266109179]
[45000,12040,0.8,1,1000,154.06036769439885,12293.373194305317,253.37319430531716]
[46000,12200,0.8,1,1000,109.02889737701142,12402.402091682328,202.40209168232832]
[47000,12500,0.8,1,1000,136.48574365208464,12538.887835334413,38.88783533441347]
[48000,12920,0.9,1,1000,631.4456781765202,13170.333513510934,250.3335135109337]
[49000,13040,0.9,1,1000,98.09136304269965,13268.424876553634,228.42487655363402]
[50000,13500,0.95,1,1000,101.84161307524957,13370.266489628884,-129.7335103711157]

{"sheet":"Shape factor","index":1,"n_rows":38,"n_cols":11,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["A subroutine for the calculation of Shape Factor"]
["Shape Factor, in the context of glacier modeling, is the ratio of the hydraulic radius to the centerline thickness."]
["The hydraulic radius, also called \"effective thickness\", is the cross-section area divided by the wetted perimenter."]
["INSTRUCTIONS: Insert required data in blue cells, data as necessary in green cells (insert lines if needed) - read F in red cell."]
["NOTE: Final contour elevation must be the same as starting elevation (=B7).  For ease of measurement, all map measurements are in mm."]
["Map scale - 1:",24000]
["Estimated ice elevation (ft)",6400]
[{"$nulls":4},"Incr. Map Dist.","Incremental Horiz. Dist. (ft)","Incremental Slope Dist. (ft)","Accumulated Horiz. Dist. (ft)","Accumulated Slope Dist. (ft)","Incremental Area (ft^2)","Accumulated Area (ft^2)"]
["Starting Elev. (ft) - =B6?",6400,"Starting Dist. (mm)",0,0,0,0,0,0,0,0]
["Next lower contour (ft)",6320,"Cumulative Dist. (mm)",18,18,1417.3228346456694,1419.5788169763719,1417.3228346456694,1419.5788169763719,56692.913385826774,56692.913385826774]
["Next lower contour (ft)",6240,"Cumulative Dist. (mm)",26,8,629.9212598425198,634.9809395577062,2047.2440944881891,2054.559756534078,100787.40157480317,157480.31496062994]
["Next lower contour (ft)",6160,"Cumulative Dist. (mm)",39,13,1023.6220472440947,1026.7434419582098,3070.8661417322837,3081.303198492288,286614.1732283465,444094.4881889764]
["Next lower contour (ft)",6080,"Cumulative Dist. (mm)",50,11,866.1417322834646,869.8284315903918,3937.0078740157483,3951.13163008268,346456.69291338586,790551.1811023622]
["Next contour (ft)",6000,"Cumulative Dist. (mm)",67,17,1338.5826771653544,1340.9711345167605,5275.5905511811025,5292.102764599441,696062.9921259843,1486614.1732283465]
["Next contour (ft)",6000,"Cumulative Dist. (mm)",90,23,1811.0236220472443,1811.0236220472443,7086.614173228347,7103.126386646685,1086614.1732283465,2573228.346456693]
["Next contour (ft)",6080,"Cumulative Dist. (mm)",120,30,2362.204724409449,2363.5590028646043,9448.818897637797,9466.685389511289,1322834.6456692915,3896062.9921259843]
["Next contour (ft)",6160,"Cumulative Dist. (mm)",135,15,1181.1023622047246,1183.808595173046,10629.921259842522,10650.493984684335,519685.0393700788,4415748.031496063]
["Next contour (ft)",6240,"Cumulative Dist. (mm)",146,11,866.1417322834646,869.8284315903918,11496.062992125986,11520.322416274726,277165.3543307087,4692913.385826771]
["Next contour (ft)",6320,"Cumulative Dist. (mm)",156,10,787.4015748031497,791.4551408655327,12283.464566929135,12311.77755714026,157480.31496062994,4850393.700787401]
["Next contour (ft)",6400,"Cumulative Dist. (mm)",165,9,708.6614173228347,713.1626773759328,12992.12598425197,13024.940234516193,56692.913385826774,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
["Next contour (ft)",null,"Cumulative Dist. (mm)",null,0,0,0,12992.12598425197,13024.940234516193,0,4907086.614173228]
[]
[]
["MINIMUM Elevation (ft)",6000,"Glacier Width = ",null,12992.12598425197,"Wetted Perimeter = ",null,13024.940234516193,"Cross-section area = ",null,4907086.614173228]
["MAXIMUM Thickness (ft)",400,null,null,null,"Hydraulic Radius (ft) =",null,376.7454226906478,"SHAPE FACTOR = ",null,0.9418635567266195]