{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["sum"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"sum","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"cut":false,"hidden":false,"merged":[[3,1,3,5],[0,0,0,7],[1,0,1,7]],"flags":["formulas_cached_only"]}
["U.S. Geological Survey Stream Gaging Measurements"]
["(from Myette and others, 1987)"]
[]
[" ","INFLOW (cfs)",{"$nulls":4},"OUTFLOW (cfs)","NET"]
["Date","Aberjona River","Aberjona Trib.","Aberjona Trib.","Aberjona Trib.","Total","Aberjona River","Gain / Loss","Comments"]
[null,"at Olympia Ave.","No. 1","No. 2","No. 3","Inflow","at Salem Street","(cfs)"]
["1985-08-29",3.02,"--","--","--",3.02,3.16,0.14000000000000012," "]
["1985-09-05",4.51,"--","--","--",4.51,4.61,0.10000000000000053]
["1985-09-13",6.62,"--","--",0.03,6.65,6.97,0.3199999999999994]
["1985-09-20",3.82,"--","--","--",3.82,3.68,-0.13999999999999968]
["1985-09-26",5.38,"--","--","--",5.38,5.8,0.41999999999999993]
["1985-10-03",5.82,"--","--","--",5.82,8.03,2.209999999999999]
["1985-10-10",6.22,"--","--","--",6.22,6.32,0.10000000000000053]
["1985-10-16",6.52,"--","--","--",6.52,7.14,0.6200000000000001]
["1985-10-29",2.96,"--","--","--",2.96,3.06,0.10000000000000009]
["1985-11-13",21.6,"--","--","--",21.6,26.7,5.099999999999998]
["1985-11-25",9.68,"--","--","--",9.68,11.5,1.8200000000000003]
["1985-12-04",11.6,0.004,0.34,0.06,12.004,13.7,1.6959999999999997,"No pumping yet at Wells G and H"]
["1985-12-04",10.9,0.004,0.33,0.06,11.294,12.5,1.2059999999999995,"First measurement with Wells G and H pumping"]
["1985-12-05",10.4,0.001,0.29,0.03,10.720999999999998,10.4,-0.32099999999999795,"Wells G and H pumping"]
["1985-12-06",10.1,"--",0.31,0.05,10.46,9.69,-0.7700000000000014,"Wells G and H pumping"]
["1985-12-09",9.53,0,0.26,0.05,9.84,9.08,-0.7599999999999998,"Wells G and H pumping"]
["1985-12-13",12.2,0.004,0.25,0.03,12.483999999999998,12.2,-0.2839999999999989,"Wells G and H pumping / rainfall in watershed"]
["1985-12-16",10.2,0.007,0.28,0.05,10.536999999999999,10.5,-0.036999999999999034,"Wells G and H pumping"]
["1985-12-18",8.87,0,0.25,0,9.12,8.27,-0.8499999999999996,"Wells G and H pumping"]
["1985-12-23",6.67,0,0.17,0,6.84,5.78,-1.0599999999999996,"Wells G and H pumping"]
["1985-12-30",5.27,0,0.08,0,5.35,3.9,-1.4499999999999997,"Wells G and H pumping"]
["1986-01-03",4.63,0,0.08,0.02,4.7299999999999995,3.47,-1.2599999999999993,"Wells G and H stop pumping after measurement"]
["1986-01-17",3.8,0,0.05,0,3.8499999999999996,3.17,-0.6799999999999997,"Wells G and H not pumping"]